(export (version D)
  (design
    (source C:\Users\Jan\Documents\Projekte\InterferometerControl\electronics\InterferometerControl\InterferometerControl.sch)
    (date "05.07.2022 09:36:53")
    (tool "Eeschema (5.1.4)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date "15 nov 2012")
        (source InterferometerControl.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref MK1)
      (value M2.5)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (libsource (lib InterferometerControl-rescue) (part Mounting_Hole-Mechanical) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5834FB2E))
    (comp (ref MK3)
      (value M2.5)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (libsource (lib InterferometerControl-rescue) (part Mounting_Hole-Mechanical) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5834FBEF))
    (comp (ref MK2)
      (value M2.5)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (libsource (lib InterferometerControl-rescue) (part Mounting_Hole-Mechanical) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5834FC19))
    (comp (ref MK4)
      (value M2.5)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (libsource (lib InterferometerControl-rescue) (part Mounting_Hole-Mechanical) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5834FC4F))
    (comp (ref P1)
      (value Conn_02x20_Odd_Even)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_02x20_Odd_Even) (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AD464A))
    (comp (ref R9)
      (value 30R)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B48B38))
    (comp (ref C1)
      (value 100p)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B4B907))
    (comp (ref Q1)
      (value Si2304)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib JA_lib) (part Si2304) (description "Leistungs-MOSFET, n-Kanal, 30 V, 3.6 A SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B5050F))
    (comp (ref U6)
      (value TS921)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib JA_lib) (part TS921) (description "Single Rail-to-Rail Input/Output Amplifiers"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B51C8E))
    (comp (ref R3)
      (value 500k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B4A05B))
    (comp (ref R6)
      (value 500)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B48608))
    (comp (ref U4)
      (value MCP4822)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/20002249B.pdf)
      (libsource (lib Analog_DAC) (part MCP4822) (description "2-Channel 12-Bit D/A Converters with SPI Interface and Internal Reference (2.048V)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B7B882))
    (comp (ref U5)
      (value MCP3204)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/21298c.pdf)
      (libsource (lib Analog_ADC) (part MCP3204) (description "A/D Converter, 12-Bit, 4-Channel, SPI Interface, 2.7V-5.5V"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B99492))
    (comp (ref U3)
      (value LM324)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/lm2902-n.pdf)
      (libsource (lib Amplifier_Operational) (part LM324) (description "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62BE7223))
    (comp (ref CON2)
      (value BNC-Multicomp)
      (footprint JA_lib:BNC-Multicomp)
      (libsource (lib JA_lib) (part BNC-Multicomp) (description BNC-Connector))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C16F10))
    (comp (ref R4)
      (value 1M)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C363FB))
    (comp (ref R5)
      (value 470k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C369F3))
    (comp (ref CON6)
      (value BNC-Multicomp)
      (footprint JA_lib:BNC-Multicomp)
      (libsource (lib JA_lib) (part BNC-Multicomp) (description BNC-Connector))
      (sheetpath (names /) (tstamps /))
      (tstamp 62CBF718))
    (comp (ref R7)
      (value 1M)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62CBF728))
    (comp (ref R8)
      (value 470k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62CBF72E))
    (comp (ref CON3)
      (value BNC-Multicomp)
      (footprint JA_lib:BNC-Multicomp)
      (libsource (lib JA_lib) (part BNC-Multicomp) (description BNC-Connector))
      (sheetpath (names /) (tstamps /))
      (tstamp 62CC6255))
    (comp (ref R1)
      (value 470k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62D1C0F8))
    (comp (ref R2)
      (value 470k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62D1C6EC))
    (comp (ref CON1)
      (value BNC-Multicomp)
      (footprint JA_lib:BNC-Multicomp)
      (libsource (lib JA_lib) (part BNC-Multicomp) (description BNC-Connector))
      (sheetpath (names /) (tstamps /))
      (tstamp 62D44A13))
    (comp (ref CON5)
      (value BNC-Multicomp)
      (footprint JA_lib:BNC-Multicomp)
      (libsource (lib JA_lib) (part BNC-Multicomp) (description BNC-Connector))
      (sheetpath (names /) (tstamps /))
      (tstamp 62D45269))
    (comp (ref U1)
      (value Teensy4.0)
      (footprint teensy:Teensy40)
      (libsource (lib teensy) (part Teensy4.0) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 62D65E6B))
    (comp (ref C4)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E6F322))
    (comp (ref C3)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E7BCBF))
    (comp (ref C5)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E7C32F))
    (comp (ref C8)
      (value 10u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E8C73D))
    (comp (ref C2)
      (value 10u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E8CBF1))
    (comp (ref C9)
      (value 10u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E8D19C))
    (comp (ref C7)
      (value 10u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E7D057))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E7C95C))
    (comp (ref J1)
      (value Conn_01x02)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62F4FE27))
    (comp (ref U7)
      (value MAX6070)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (libsource (lib JA_lib) (part MAX6070) (description "Low-Noise, High-Precision Series, 3V, SOT-23-6"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62FD405C))
    (comp (ref C10)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 63017C9D))
    (comp (ref J2)
      (value Conn_01x02)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 63037DEC))
    (comp (ref U8)
      (value MAX11270)
      (footprint Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm)
      (libsource (lib JA_lib) (part MCP11270) (description "24bit ADC with Integrated PGA, TSSOP-24"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C0CB9C))
    (comp (ref R10)
      (value 5k1)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C85B61))
    (comp (ref R12)
      (value 5k1)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C86736))
    (comp (ref R11)
      (value 97k6)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C86B0F))
    (comp (ref J3)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62C87495))
    (comp (ref C12)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E158C5))
    (comp (ref C13)
      (value 10u)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62E3CD40))
    (comp (ref U2)
      (value LM4871)
      (footprint Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm)
      (libsource (lib JA_lib) (part LM4871) (description "Boomer 3W Audio Power Amplifier with Shutdown Mode, SOIC-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 63063851))
    (comp (ref C11)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 630A3712)))
  (libparts
    (libpart (lib Amplifier_Operational) (part LM2902)
      (aliases
        (alias LM324)
        (alias TLC274)
        (alias TLC279)
        (alias TL074)
        (alias LM324A)
        (alias MCP6004)
        (alias TL084)
        (alias TL064)
        (alias LMV324)
        (alias LMC6484)
        (alias MCP604)
        (alias MC33079)
        (alias MC33174)
        (alias MC33179)
        (alias OPA1604)
        (alias OPA1679)
        (alias OPA4134)
        (alias OPA4340UA)
        (alias OPA4376)
        (alias MCP6L94)
        (alias TSV914)
        (alias ADA4807-4)
        (alias TSV994))
      (description "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14")
      (docs http://www.ti.com/lit/ds/symlink/lm2902-n.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*)
        (fp SSOP*5.3x6.2mm*P0.65mm*)
        (fp MSOP*3x3mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2902))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib Analog_ADC) (part MCP3204)
      (description "A/D Converter, 12-Bit, 4-Channel, SPI Interface, 2.7V-5.5V")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/21298c.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP3204))
      (pins
        (pin (num 1) (name CH0) (type input))
        (pin (num 2) (name CH1) (type input))
        (pin (num 3) (name CH2) (type input))
        (pin (num 4) (name CH3) (type input))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name NC) (type NotConnected))
        (pin (num 7) (name DGND) (type power_in))
        (pin (num 8) (name ~CS~/SHDN) (type input))
        (pin (num 9) (name Din) (type input))
        (pin (num 10) (name Dout) (type output))
        (pin (num 11) (name CLK) (type input))
        (pin (num 12) (name AGND) (type power_in))
        (pin (num 13) (name Vref) (type power_in))
        (pin (num 14) (name Vdd) (type power_in))))
    (libpart (lib Analog_DAC) (part MCP4802)
      (aliases
        (alias MCP4812)
        (alias MCP4822))
      (description "2-Channel 8-Bit D/A Converters with SPI Interface and Internal Reference (2.048V)")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/20002249B.pdf)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x4.9mm*P1.27mm*)
        (fp MSOP*3x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP4802))
      (pins
        (pin (num 1) (name Vdd) (type power_in))
        (pin (num 2) (name ~CS) (type input))
        (pin (num 3) (name SCK) (type input))
        (pin (num 4) (name SDI) (type input))
        (pin (num 5) (name ~LDAC) (type input))
        (pin (num 6) (name VB) (type output))
        (pin (num 7) (name Vss) (type power_in))
        (pin (num 8) (name VA) (type output))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x03)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib InterferometerControl-rescue) (part Mounting_Hole-Mechanical)
      (footprints
        (fp Mounting?Hole*)
        (fp Hole*))
      (fields
        (field (name Reference) MK)
        (field (name Value) Mounting_Hole-Mechanical)))
    (libpart (lib JA_lib) (part BNC-Multicomp)
      (description BNC-Connector)
      (fields
        (field (name Reference) CON)
        (field (name Value) BNC-Multicomp)
        (field (name Footprint) JA_lib:BNC-Multicomp))
      (pins
        (pin (num 1) (name SIG) (type BiDi))
        (pin (num 2) (name GND) (type BiDi))))
    (libpart (lib JA_lib) (part LM4871)
      (description "Boomer 3W Audio Power Amplifier with Shutdown Mode, SOIC-8")
      (footprints
        (fp SO*8))
      (fields
        (field (name Reference) U)
        (field (name Value) LM4871))
      (pins
        (pin (num 1) (name SHDN) (type input))
        (pin (num 2) (name BYPASS) (type passive))
        (pin (num 3) (name VIN+) (type input))
        (pin (num 4) (name VIN-) (type input))
        (pin (num 5) (name VOUT1) (type output))
        (pin (num 6) (name VDD) (type power_in))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name VOUT2) (type output))))
    (libpart (lib JA_lib) (part MAX6070)
      (aliases
        (alias REF3220AMDBVREP)
        (alias REF3225AMDBVREP)
        (alias REF3230AMDBVREP)
        (alias REF3233AMDBVREP)
        (alias REF3240AMDBVREP))
      (description "Low-Noise, High-Precision Series, 3V, SOT-23-6")
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) MAX6070)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name FILTER) (type power_in))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name ENABLE) (type input))
        (pin (num 4) (name VIN) (type power_in))
        (pin (num 5) (name OUT_S) (type input))
        (pin (num 6) (name OUT_F) (type output))))
    (libpart (lib JA_lib) (part MCP11270)
      (description "24bit ADC with Integrated PGA, TSSOP-24")
      (footprints
        (fp TSSOP*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP11270))
      (pins
        (pin (num 1) (name DIN) (type input))
        (pin (num 2) (name DOUT) (type output))
        (pin (num 3) (name DGND) (type power_in))
        (pin (num 4) (name SYNC) (type input))
        (pin (num 5) (name RSTB) (type input))
        (pin (num 6) (name GPIO3) (type BiDi))
        (pin (num 7) (name GPIO2) (type BiDi))
        (pin (num 8) (name GPIO1) (type BiDi))
        (pin (num 9) (name AVDD) (type power_in))
        (pin (num 10) (name AVSS) (type power_in))
        (pin (num 11) (name AINN) (type power_in))
        (pin (num 12) (name AINP) (type power_in))
        (pin (num 13) (name REFN) (type power_in))
        (pin (num 14) (name REFP) (type power_in))
        (pin (num 15) (name CAPN) (type power_in))
        (pin (num 16) (name CAPP) (type power_in))
        (pin (num 18) (name RDYB) (type BiDi))
        (pin (num 19) (name CLK) (type BiDi))
        (pin (num 20) (name DGND) (type power_in))
        (pin (num 21) (name CAPREG) (type power_out))
        (pin (num 22) (name DVDD) (type input))
        (pin (num 23) (name CSB) (type input))
        (pin (num 24) (name SCLK) (type input))))
    (libpart (lib JA_lib) (part Si2304)
      (description "Leistungs-MOSFET, n-Kanal, 30 V, 3.6 A SOT-23")
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) Si2304)
        (field (name Spice_Primitive) Q)
        (field (name Spice_Model) Si2304DDS)
        (field (name Spice_Netlist_Enabled) Y)
        (field (name Spice_Lib_File) "C:\\Users\\Jan\\Downloads\\si2304dds_ps_revb\\Si2304DDS_PS Rev B.lib"))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib JA_lib) (part TS921)
      (description "Single Rail-to-Rail Input/Output Amplifiers")
      (footprints
        (fp SOIC?8*))
      (fields
        (field (name Reference) U)
        (field (name Value) TS921))
      (pins
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name V+) (type power_in))))
    (libpart (lib teensy) (part Teensy4.0)
      (fields
        (field (name Reference) U)
        (field (name Value) Teensy4.0))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name 0_RX1_CRX2_CS1) (type BiDi))
        (pin (num 3) (name 1_TX1_CTX2_MISO1) (type BiDi))
        (pin (num 4) (name 2_OUT2) (type BiDi))
        (pin (num 5) (name 3_LRCLK2) (type BiDi))
        (pin (num 6) (name 4_BCLK2) (type BiDi))
        (pin (num 7) (name 5_IN2) (type BiDi))
        (pin (num 8) (name 6_OUT1D) (type BiDi))
        (pin (num 9) (name 7_RX2_OUT1A) (type BiDi))
        (pin (num 10) (name 8_TX2_IN1) (type BiDi))
        (pin (num 11) (name 9_OUT1C) (type BiDi))
        (pin (num 12) (name 10_CS_MQSR) (type BiDi))
        (pin (num 13) (name 11_MOSI_CTX1) (type BiDi))
        (pin (num 14) (name 12_MISO_MQSL) (type BiDi))
        (pin (num 15) (name VBAT) (type power_in))
        (pin (num 16) (name 3V3) (type power_in))
        (pin (num 17) (name GND) (type power_in))
        (pin (num 18) (name PROGRAM) (type input))
        (pin (num 19) (name ON_OFF) (type input))
        (pin (num 20) (name 13_SCK_CRX1_LED) (type BiDi))
        (pin (num 21) (name 14_A0_TX3_SPDIF_OUT) (type BiDi))
        (pin (num 22) (name 15_A1_RX3_SPDIF_IN) (type BiDi))
        (pin (num 23) (name 16_A2_RX4_SCL1) (type BiDi))
        (pin (num 24) (name 17_A3_TX4_SDA1) (type BiDi))
        (pin (num 25) (name 18_A4_SDA0) (type BiDi))
        (pin (num 26) (name 19_A5_SCL0) (type BiDi))
        (pin (num 27) (name 20_A6_TX5_LRCLK1) (type BiDi))
        (pin (num 28) (name 21_A7_RX5_BCLK1) (type BiDi))
        (pin (num 29) (name 22_A8_CTX1) (type BiDi))
        (pin (num 30) (name 23_A9_CRX1_MCLK1) (type BiDi))
        (pin (num 31) (name 3V3) (type power_out))
        (pin (num 32) (name GND) (type power_in))
        (pin (num 33) (name VIN) (type power_in))
        (pin (num 34) (name VUSB) (type power_out))
        (pin (num 35) (name 24_A10_TX6_SCL2) (type BiDi))
        (pin (num 36) (name 25_A11_RX6_SDA2) (type BiDi))
        (pin (num 37) (name 26_A12_MOSI1) (type BiDi))
        (pin (num 38) (name 27_A13_SCK1) (type BiDi))
        (pin (num 39) (name 28_RX7) (type BiDi))
        (pin (num 40) (name 29_TX7) (type BiDi))
        (pin (num 41) (name 30_CRX3) (type BiDi))
        (pin (num 42) (name 31_CTX3) (type BiDi))
        (pin (num 43) (name 32_OUT1B) (type BiDi))
        (pin (num 44) (name 33_MCLK2) (type BiDi))
        (pin (num 45) (name 34_DAT1_MISO2) (type BiDi))
        (pin (num 46) (name 35_DAT0_MOSI2) (type BiDi))
        (pin (num 47) (name GND) (type power_out))
        (pin (num 48) (name 36_CLK_CS2) (type BiDi))
        (pin (num 49) (name 3V3) (type power_out))
        (pin (num 50) (name 37_CMD_SCK2) (type BiDi))
        (pin (num 51) (name 38_DAT3_RX5) (type BiDi))
        (pin (num 52) (name 39_DAT2_TX5) (type BiDi))
        (pin (num 53) (name D-) (type BiDi))
        (pin (num 54) (name D+) (type BiDi)))))
  (libraries
    (library (logical Amplifier_Operational)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Amplifier_Operational.lib"))
    (library (logical Analog_ADC)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Analog_ADC.lib"))
    (library (logical Analog_DAC)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Analog_DAC.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical InterferometerControl-rescue)
      (uri C:\Users\Jan\Documents\Projekte\InterferometerControl\electronics\InterferometerControl/InterferometerControl-rescue.lib))
    (library (logical JA_lib)
      (uri C:/Users/Jan/Documents/Elektronik/JA_lib.lib))
    (library (logical teensy)
      (uri C:\Users\Jan\Documents\Projekte\InterferometerControl\electronics\InterferometerControl/teensy_library/teensy.lib)))
  (nets
    (net (code 1) (name /TEENSY_A0)
      (node (ref U3) (pin 2))
      (node (ref U1) (pin 21))
      (node (ref U5) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 2) (name /TEENY_A1)
      (node (ref U3) (pin 6))
      (node (ref U3) (pin 7))
      (node (ref U1) (pin 22))
      (node (ref U5) (pin 2)))
    (net (code 3) (name /TEENY_A2)
      (node (ref U3) (pin 8))
      (node (ref U5) (pin 3))
      (node (ref U3) (pin 9))
      (node (ref U1) (pin 23)))
    (net (code 4) (name /TEENY_A3)
      (node (ref U1) (pin 24))
      (node (ref U3) (pin 13))
      (node (ref U3) (pin 14))
      (node (ref U5) (pin 4)))
    (net (code 5) (name +3V3)
      (node (ref U1) (pin 16))
      (node (ref P1) (pin 1))
      (node (ref U5) (pin 14))
      (node (ref P1) (pin 17))
      (node (ref C2) (pin 1))
      (node (ref U8) (pin 9))
      (node (ref C4) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref U8) (pin 22)))
    (net (code 6) (name /Vref)
      (node (ref R10) (pin 1))
      (node (ref U7) (pin 5))
      (node (ref U5) (pin 13))
      (node (ref U8) (pin 14))
      (node (ref J2) (pin 1))
      (node (ref U7) (pin 6))
      (node (ref R12) (pin 1)))
    (net (code 7) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref U3) (pin 12)))
    (net (code 8) (name GND)
      (node (ref P1) (pin 30))
      (node (ref CON2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 7))
      (node (ref U8) (pin 10))
      (node (ref R11) (pin 2))
      (node (ref J3) (pin 3))
      (node (ref C10) (pin 2))
      (node (ref U5) (pin 7))
      (node (ref U8) (pin 20))
      (node (ref U8) (pin 3))
      (node (ref U8) (pin 13))
      (node (ref CON6) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref CON3) (pin 2))
      (node (ref U4) (pin 7))
      (node (ref U6) (pin 4))
      (node (ref P1) (pin 25))
      (node (ref P1) (pin 20))
      (node (ref R8) (pin 1))
      (node (ref P1) (pin 14))
      (node (ref P1) (pin 9))
      (node (ref P1) (pin 6))
      (node (ref P1) (pin 39))
      (node (ref U3) (pin 11))
      (node (ref R9) (pin 1))
      (node (ref P1) (pin 34))
      (node (ref R5) (pin 1))
      (node (ref U5) (pin 12))
      (node (ref C5) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U7) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C13) (pin 1))
      (node (ref U1) (pin 32))
      (node (ref C9) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2)))
    (net (code 9) (name +5V)
      (node (ref U1) (pin 34))
      (node (ref C6) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref U6) (pin 7))
      (node (ref P1) (pin 2))
      (node (ref P1) (pin 4))
      (node (ref U3) (pin 4))
      (node (ref C8) (pin 1))
      (node (ref CON5) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref C5) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U7) (pin 4))
      (node (ref U7) (pin 3)))
    (net (code 10) (name "Net-(U1-Pad40)")
      (node (ref U1) (pin 40)))
    (net (code 11) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 12) (name "Net-(U1-Pad31)")
      (node (ref U1) (pin 31)))
    (net (code 13) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 14) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 15) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36)))
    (net (code 16) (name "Net-(U1-Pad37)")
      (node (ref U1) (pin 37)))
    (net (code 17) (name "Net-(U1-Pad38)")
      (node (ref U1) (pin 38)))
    (net (code 18) (name "Net-(U1-Pad39)")
      (node (ref U1) (pin 39)))
    (net (code 19) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 20) (name "Net-(U1-Pad41)")
      (node (ref U1) (pin 41)))
    (net (code 21) (name "Net-(U1-Pad42)")
      (node (ref U1) (pin 42)))
    (net (code 22) (name "Net-(U1-Pad43)")
      (node (ref U1) (pin 43)))
    (net (code 23) (name "Net-(U1-Pad44)")
      (node (ref U1) (pin 44)))
    (net (code 24) (name "Net-(U1-Pad45)")
      (node (ref U1) (pin 45)))
    (net (code 25) (name "Net-(U1-Pad46)")
      (node (ref U1) (pin 46)))
    (net (code 26) (name "Net-(U1-Pad47)")
      (node (ref U1) (pin 47)))
    (net (code 27) (name "Net-(U1-Pad48)")
      (node (ref U1) (pin 48)))
    (net (code 28) (name "Net-(U1-Pad49)")
      (node (ref U1) (pin 49)))
    (net (code 29) (name "Net-(U1-Pad19)")
      (node (ref U1) (pin 19)))
    (net (code 30) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 31) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 32) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 33) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 34) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 35) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 36) (name "Net-(U1-Pad25)")
      (node (ref U1) (pin 25)))
    (net (code 37) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 38) (name "Net-(U1-Pad27)")
      (node (ref U1) (pin 27)))
    (net (code 39) (name "Net-(U1-Pad28)")
      (node (ref U1) (pin 28)))
    (net (code 40) (name "/GPIO11(SPI0_SCK)")
      (node (ref P1) (pin 23))
      (node (ref U1) (pin 20))
      (node (ref U4) (pin 3)))
    (net (code 41) (name "/GPIO10(SPI0_MOSI)")
      (node (ref U4) (pin 4))
      (node (ref U1) (pin 13))
      (node (ref P1) (pin 19)))
    (net (code 42) (name "/GPIO8(SPI0_CE_N)")
      (node (ref U1) (pin 12))
      (node (ref P1) (pin 24))
      (node (ref U4) (pin 2)))
    (net (code 43) (name /GPIO5)
      (node (ref U1) (pin 7))
      (node (ref U4) (pin 5))
      (node (ref P1) (pin 29)))
    (net (code 44) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 45) (name "Net-(U1-Pad50)")
      (node (ref U1) (pin 50)))
    (net (code 46) (name "Net-(U1-Pad51)")
      (node (ref U1) (pin 51)))
    (net (code 47) (name "Net-(U1-Pad52)")
      (node (ref U1) (pin 52)))
    (net (code 48) (name "Net-(U1-Pad53)")
      (node (ref U1) (pin 53)))
    (net (code 49) (name "Net-(U1-Pad54)")
      (node (ref U1) (pin 54)))
    (net (code 50) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 51) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 52) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 53) (name "/GPIO27(GEN2)")
      (node (ref P1) (pin 13))
      (node (ref U1) (pin 6))
      (node (ref U8) (pin 4)))
    (net (code 54) (name "/GPIO22(GEN3)")
      (node (ref U1) (pin 5))
      (node (ref U8) (pin 5))
      (node (ref P1) (pin 15)))
    (net (code 55) (name "Net-(C12-Pad1)")
      (node (ref U8) (pin 15))
      (node (ref C12) (pin 1)))
    (net (code 56) (name "Net-(C12-Pad2)")
      (node (ref U8) (pin 16))
      (node (ref C12) (pin 2)))
    (net (code 57) (name "Net-(U8-Pad19)")
      (node (ref U8) (pin 19)))
    (net (code 58) (name "Net-(C13-Pad2)")
      (node (ref C13) (pin 2))
      (node (ref U8) (pin 21)))
    (net (code 59) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref R12) (pin 2)))
    (net (code 60) (name /ch0)
      (node (ref U8) (pin 11))
      (node (ref J3) (pin 2)))
    (net (code 61) (name "Net-(U8-Pad8)")
      (node (ref U8) (pin 8)))
    (net (code 62) (name "Net-(U8-Pad7)")
      (node (ref U8) (pin 7)))
    (net (code 63) (name "Net-(U8-Pad6)")
      (node (ref U8) (pin 6)))
    (net (code 64) (name "Net-(R1-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 65) (name "Net-(C11-Pad1)")
      (node (ref C11) (pin 1))
      (node (ref U2) (pin 2)))
    (net (code 66) (name "Net-(CON1-Pad1)")
      (node (ref U2) (pin 5))
      (node (ref R1) (pin 2))
      (node (ref CON1) (pin 1)))
    (net (code 67) (name "Net-(CON1-Pad2)")
      (node (ref U2) (pin 8))
      (node (ref CON1) (pin 2)))
    (net (code 68) (name /GPIO6)
      (node (ref U8) (pin 18))
      (node (ref U1) (pin 8))
      (node (ref P1) (pin 31)))
    (net (code 69) (name "Net-(C10-Pad1)")
      (node (ref U7) (pin 1))
      (node (ref C10) (pin 1)))
    (net (code 70) (name "/GPIO21(SPI1_SCK)")
      (node (ref U5) (pin 11))
      (node (ref P1) (pin 40))
      (node (ref U8) (pin 24)))
    (net (code 71) (name /ch1)
      (node (ref U8) (pin 12))
      (node (ref R10) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 72) (name "/GPIO19(SPI1_MISO)")
      (node (ref U5) (pin 10))
      (node (ref P1) (pin 35))
      (node (ref U8) (pin 2)))
    (net (code 73) (name "/GPIO20(SPI1_MOSI)")
      (node (ref U8) (pin 1))
      (node (ref U5) (pin 9))
      (node (ref P1) (pin 38)))
    (net (code 74) (name "/GPIO17(GEN0)")
      (node (ref P1) (pin 11))
      (node (ref U1) (pin 9))
      (node (ref U8) (pin 23)))
    (net (code 75) (name "/GPIO2(SDA1)")
      (node (ref P1) (pin 3)))
    (net (code 76) (name "/GPIO13(PWM1)")
      (node (ref P1) (pin 33)))
    (net (code 77) (name /ID_SD)
      (node (ref P1) (pin 27)))
    (net (code 78) (name "/GPIO3(SCL1)")
      (node (ref P1) (pin 5)))
    (net (code 79) (name "/GPIO4(GCLK)")
      (node (ref P1) (pin 7)))
    (net (code 80) (name "/GPIO9(SPI0_MISO)")
      (node (ref P1) (pin 21)))
    (net (code 81) (name "Net-(C1-Pad1)")
      (node (ref U6) (pin 6))
      (node (ref C1) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 82) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 83) (name "Net-(C1-Pad2)")
      (node (ref U6) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref C1) (pin 2)))
    (net (code 84) (name "Net-(Q1-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref Q1) (pin 2)))
    (net (code 85) (name "Net-(CON5-Pad2)")
      (node (ref Q1) (pin 3))
      (node (ref CON5) (pin 2)))
    (net (code 86) (name "/GPIO12(PWM0)")
      (node (ref P1) (pin 32)))
    (net (code 87) (name /GPIO26)
      (node (ref P1) (pin 37)))
    (net (code 88) (name /GPIO16)
      (node (ref P1) (pin 36)))
    (net (code 89) (name /ID_SC)
      (node (ref P1) (pin 28)))
    (net (code 90) (name "/GPIO7(SPI1_CE_N)")
      (node (ref P1) (pin 26))
      (node (ref U5) (pin 8)))
    (net (code 91) (name "/GPIO25(GEN6)")
      (node (ref P1) (pin 22)))
    (net (code 92) (name "/GPIO24(GEN5)")
      (node (ref P1) (pin 18)))
    (net (code 93) (name "/GPIO23(GEN4)")
      (node (ref P1) (pin 16)))
    (net (code 94) (name "/GPIO18(GEN1)(PWM0)")
      (node (ref P1) (pin 12)))
    (net (code 95) (name "/GPIO15(RXD0)")
      (node (ref P1) (pin 10)))
    (net (code 96) (name "/GPIO14(TXD0)")
      (node (ref P1) (pin 8)))
    (net (code 97) (name "Net-(CON2-Pad1)")
      (node (ref R4) (pin 2))
      (node (ref CON2) (pin 1)))
    (net (code 98) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref R8) (pin 2)))
    (net (code 99) (name "Net-(CON6-Pad1)")
      (node (ref CON6) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 100) (name "Net-(R4-Pad1)")
      (node (ref U3) (pin 3))
      (node (ref R4) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 101) (name "Net-(CON3-Pad1)")
      (node (ref U3) (pin 10))
      (node (ref CON3) (pin 1)))
    (net (code 102) (name /DAC2)
      (node (ref U4) (pin 6))
      (node (ref U2) (pin 3)))
    (net (code 103) (name "Net-(U4-Pad8)")
      (node (ref U4) (pin 8))
      (node (ref U6) (pin 3)))
    (net (code 104) (name "Net-(U5-Pad5)")
      (node (ref U5) (pin 5)))
    (net (code 105) (name "Net-(U5-Pad6)")
      (node (ref U5) (pin 6)))))