
(rules PCB InterferometerControl
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 1601)
    (layer_rule F.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.2)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 1.9)
    )
  )
  (rule
    (width 200.0)
    (clear 200.2)
    (clear 100.0 (type smd_to_turn_gap))
    (clear 50.0 (type smd_smd))
  )
  (padstack "Via[0-1]_900:600_um"
    (shape
      (circle F.Cu 900.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 900.0 0.0 0.0)
    )
    (attach off)
  )
  (padstack "Via[0-1]_1000:700_um"
    (shape
      (circle F.Cu 1000.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 1000.0 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_900:600_um" "Via[0-1]_900:600_um" default
  )
  (via 
    "Via[0-1]_1000:700_um" "Via[0-1]_1000:700_um" default
  )
  (via 
    "Via[0-1]_900:600_um-kicad_default" "Via[0-1]_900:600_um" "kicad_default"
  )
  (via 
    "Via[0-1]_1000:700_um-kicad_default" "Via[0-1]_1000:700_um" "kicad_default"
  )
  (via 
    "Via[0-1]_900:600_um-Power" "Via[0-1]_900:600_um" Power
  )
  (via 
    "Via[0-1]_1000:700_um-Power" "Via[0-1]_1000:700_um" Power
  )
  (via_rule
    default "Via[0-1]_900:600_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_900:600_um-kicad_default"
  )
  (via_rule
    Power "Via[0-1]_1000:700_um-Power"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 200.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    +3V3 +5V GND "/ID_SD" "/ID_SC" /GPIO5 /GPIO6 /GPIO26
    "/GPIO2(SDA1)" "/GPIO3(SCL1)" "/GPIO4(GCLK)" "/GPIO14(TXD0)" "/GPIO15(RXD0)" "/GPIO17(GEN0)" "/GPIO27(GEN2)" "/GPIO22(GEN3)"
    "/GPIO23(GEN4)" "/GPIO24(GEN5)" "/GPIO25(GEN6)" "/GPIO18(GEN1)(PWM0)" "/GPIO10(SPI0_MOSI)" "/GPIO9(SPI0_MISO)" "/GPIO11(SPI0_SCK)" "/GPIO8(SPI0_CE_N)"
    "/GPIO7(SPI1_CE_N)" "/GPIO12(PWM0)" "/GPIO13(PWM1)" "/GPIO19(SPI1_MISO)" /GPIO16 "/GPIO20(SPI1_MOSI)" "/GPIO21(SPI1_SCK)" "Net-(C1-Pad1)"
    "Net-(C1-Pad2)" "Net-(Q1-Pad1)" "Net-(Q1-Pad2)" "Net-(CON5-Pad2)" "Net-(CON1-Pad1)" "Net-(R1-Pad1)" "Net-(CON2-Pad1)" "Net-(R4-Pad1)"
    "Net-(R7-Pad1)" "Net-(CON6-Pad1)" "Net-(U1-Pad17)" "Net-(U1-Pad18)" "Net-(U1-Pad19)" "Net-(U1-Pad15)" "Net-(U1-Pad14)" "/TEENSY_A0"
    "/TEENY_A1" "/TEENY_A2" "/TEENY_A3" "Net-(U1-Pad25)" "Net-(U1-Pad26)" "Net-(U1-Pad27)" "Net-(U1-Pad28)" "Net-(U1-Pad29)"
    "Net-(U1-Pad30)" "Net-(U1-Pad31)" "Net-(U1-Pad33)" "Net-(U1-Pad11)" "Net-(U1-Pad10)" "Net-(U1-Pad4)" "Net-(U1-Pad3)" "Net-(U1-Pad2)"
    "Net-(U1-Pad1)" "Net-(U1-Pad35)" "Net-(U1-Pad36)" "Net-(U1-Pad37)" "Net-(U1-Pad38)" "Net-(U1-Pad39)" "Net-(U1-Pad40)" "Net-(U1-Pad41)"
    "Net-(U1-Pad42)" "Net-(U1-Pad43)" "Net-(U1-Pad44)" "Net-(CON3-Pad1)" "Net-(U4-Pad8)" "Net-(U5-Pad5)" "Net-(U5-Pad6)" "Net-(J1-Pad1)"
    "Net-(C10-Pad1)" /Vref "Net-(C11-Pad1)" "Net-(C12-Pad1)" "Net-(C12-Pad2)" "Net-(C13-Pad2)" "Net-(CON1-Pad2)" "Net-(J3-Pad1)"
    /ch0 /ch1 /DAC2 "Net-(U8-Pad6)" "Net-(U8-Pad7)" "Net-(U8-Pad8)" "Net-(U8-Pad19)"
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 200.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class Power
    (clearance_class Power)
    (via_rule Power)
    (rule
      (width 500.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)